{"text_format":"2","workbook":"xls","n_sheets":2,"sheets":["Emitterschaltung mit Stromgegenkopplung","Kollektorschaltung"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Emitterschaltung mit Stromgegenkopplung","index":0,"n_rows":34,"n_cols":37,"rows_kept":34,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
[null,"Parameter","Wert","Einheit","Beschreibung"]
[null,"U B",9,"Volt","Betriebsspannung",{"$nulls":31},"U B"]
[null,"Transistor","BC548"]
[null,"I C",0.011,"Ampere","siehe Datenblatt",{"$nulls":14},"R 1",{"$nulls":10},"R C"]
[null,"I B",5e-05,"Ampere","siehe Datenblatt"]
[null,"B",219.99999999999997,"fach","Stromverstärkung"]
[null,"U BE",0.7,"Volt"]
[null,"I Q / I B",8.6,"fach","(2-10 fach)"]
[null,"U CE",1,"Volt","ca. 1V",{"$nulls":29},"C OUT"]
[null,"U RE",1.1,"Volt","1-2V oder max. UB/10",{"$nulls":31},"Ausgang"]
[null,"U CE ~ U RE",3.141592654,{"$nulls":28},"+",null,"-"]
[null,"f u",20,"Hz","untere Grenzfrequenz"]
[{"$nulls":28},"Kollektor"]
[null,"I E",0.011049999999999999,"Ampere",{"$nulls":10},"C IN",{"$nulls":7},"Basis"]
[null,"R E",99.5,"Ohm","ca. 10-1000 Ohm",null,null,null,"Eingang",{"$nulls":17},"T 1"]
[null,"U RC",3.45,"Volt",{"$nulls":7},"-",null,"+"]
[null,"R C",313.6,"Ohm"]
[null,"V",3.2,"fach","Spannungsverstärkung",{"$nulls":21},"_|",null,"Emitter"]
[null,"U R2",1.8,"Volt"]
[null,"I R2",0.00043,"Ampere"]
[null,"R 2",4186,"Ohm","aufrunden"]
[null,"R 1",15000.000000000002,"Ohm","abrunden",{"$nulls":14},"R 2",{"$nulls":5},"R E",{"$nulls":8},"R 3"]
[null,"R IN",21889.999999999996,"Ohm"]
[null,"R OUT",313.6,"Ohm","ist etwas größer"]
[null,"C IN",364,"nF"]
[null,"C OUT",25375,"nF","1000nF = 1µF"]
[null,"C 1",25375,"nF","kann auch etwas kleiner sein"]
[null,"R 3",1592,"Ohm","10-20 mal „R E“"]
[{"$nulls":34},"C 1"]
[]
[]
[{"$nulls":8},"0 V"]
[]
[{"$nulls":36},"0 V"]

{"sheet":"Kollektorschaltung","index":1,"n_rows":29,"n_cols":37,"rows_kept":29,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
[null,"Parameter","Wert","Einheit","Beschreibung"]
[null,"U B",9,"Volt","Betriebsspannung",{"$nulls":31},"U B"]
[null,"Transistor","BC548"]
[null,"I C",0.011,"Ampere","siehe Datenblatt",{"$nulls":14},"R 1"]
[null,"I B",5e-05,"Ampere","siehe Datenblatt"]
[null,"B",219.99999999999997,"fach","Stromverstärkung"]
[null,"U BE",0.7,"Volt"]
[null,"I Q / I B",10,"fach","(2-10 fach)"]
[null,"U CE",1,"Volt","ca. 1V"]
[null,"U RE",1.1,"Volt","1-2V oder max. UB/10"]
[null,"U CE ~ U RE",3.141592654]
[null,"f u",20,"Hz","untere Grenzfrequenz"]
[{"$nulls":28},"Kollektor"]
[null,"I E",0.011049999999999999,"Ampere",{"$nulls":10},"C IN",{"$nulls":7},"Basis"]
[null,"R E",99.5,"Ohm","ca. 10-1000 Ohm",null,null,null,"Eingang",{"$nulls":17},"T 1"]
[null,"V",0.92,"fach","Spannungsverstärkung",{"$nulls":6},"-",null,"+"]
[null,"R 1 = R 2",9000,"Ohm"]
[{"$nulls":26},"_|",null,"Emitter"]
[null,"R IN",21889.999999999996,"Ohm","ist etwas kleiner",{"$nulls":29},"C OUT"]
[null,"R OUT",99.5,"Ohm","ist etwas größer"]
[null,"C IN",364,"nF",{"$nulls":27},"+",null,"-",null,null,"Ausgang"]
[null,"C OUT",79977,"nF","1000nF = 1µF",{"$nulls":14},"R 2",{"$nulls":10},"R E"]
[]
[]
[]
[]
[]
[]
[{"$nulls":8},"0 V",{"$nulls":27},"0 V"]